**TEMPOMATIC WC direct flush valve**

Electronic mains supply - sea water compatible

Cross wall for walls ≤ 30mm

Reference: **463030HK**

Specification description

Flush system without cistern: directly connected to pipework.

Mains supply with 1" solenoid valve.

230/12V transformer.

IP65 electronic housing unit.

For cross wall installation on walls ≤ 30mm.

Shock-resistant infrared presence detection sensor.

Voluntary activation (when hand is detected ~10cm in front of the sensor) or automatic flush when the user leaves.

Time flow ~7 seconds can be adjusted from 3 - 12 seconds.

Detection distance, flow rate and flush volume can be adjusted.

Connection washer Ø 32/55mm.

Wall plate flush to the wall.

Threaded rod can be cut to size.

Base flow rate: 1 L/sec.

Suitable for rimless WC pans.

Sea water compatible.

30-year warranty.