**AZA Urinal divider**

Matte black 304 stainless steel - H. 600mm

Reference: **100620BK**

Specification description

Urinal divider for wall-mounting.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 3mm.

Matte black Teflon® finish.

Rounded edges.

Supplied with fixing elements and TORX anti-theft screws.

Weight: 4kg.

30-year warranty.