**HEMI inset washbasin Ø 385mm**

Matte black 304 stainless steel - Inset from above or below

Reference: **120490BK**

Specification description

Round washbasin for recessed installation from above or below.

Basin internal diameter: 385mm.

Cut-out diameter: 400mm for installation from above, 380mm for installation from below.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 0.8mm.

Matte black Teflon® finish.

One-piece, seam-free pressed bowl.

Rounded edges prevent injury.

Supplied without waste. Waste with black finish can be added (6110BK) or chrome finish (6110).

Without overflow.

CE marked. Complies with European standard EN 14688.

Weight: 1.6kg.

30-year warranty.