**Mechanical mixer with retracting hand spray**

Single hole mechanical mixer with retracting hand spray

Mixer with Hygiene control lever

Reference: **2211L**

Specification description

Deck-mounted mechanical sink mixer suitable for baby baths.

Single hole mixer with retracting hand spray with swivelling spout H. 105mm L. 200mm.

Ø 40mm standard ceramic cartridge with pre-set maximum temperature limiter.

Securitouch thermal insulation prevents burns.

Mechanical mixer with retracting hand spray with 2 jet options: flow straightener/rain effect.

Body with smooth interior.

Flow rate limited to 7 lpm at 3 bar.

Chrome-plated brass body and Hygiene control lever L. 175mm.

BIOSAFE flexible shower hose reduces bacterial proliferation: transparent polyurethane flexible hose ensures replacement if biofilm is present, smooth interior and exterior.

Narrow flexible (interior Ø 6mm), low water volume.

Specific counterweight.

PEX flexibles F⅜".

Fixing reinforced by 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

30-year warranty.