**Stainless steel drop-down rail with leg, bright, L. 650mm**

UltraPolish bright polished stainless steel

Ø 32mm

Reference: **510162P**

Specification description

Drop-down grab bar Ø 32mm with leg, for people with reduced mobility.

Drop-down grab bar for WCs or showers.

Allows side access in the raised position.

In the lowered position use as a grab bar, for standing up and assisting movement.

With automatic folding leg: to be used as reinforcement when the wall fixing alone is insufficient.

Leg height can be adjusted from 760 - 780mm.

Retained in upright position. Slowed down descent.

Drop-down grab bar made from bacteriostatic 304 stainless steel tube.

Stainless steel with UltraPolish bright polished finish, uniform non-porous surface for easy maintenance and hygiene.

Fixings concealed by a 4mm thick 304 stainless steel cover plate.

Supplied with stainless steel screws for concrete walls.

Dimensions: 650 x 800 x 105mm.

Tested to over 250kg. Maximum recommended user weight 170kg.

30-year warranty.

CE marked.