**Mechanical mixer with retracting hand spray**

Single hole mechanical mixer with retracting hand spray

Mixer with swivelling swan neck spout

Reference: **2597**

Specification description

Deck-mounted mechanical mixer with retracting hand spray.

Single hole mixer with swivelling swan neck spout H. 210mm L. 210mm.

Mechanical mixer with scale resistant hand spray with 3 spray options: laminar flow, rain-effect and blade.

Ø 40mm standard ceramic cartridge with pre-set maximum temperature limiter.

Flow rate 5 lpm at 3 bar.

Chrome-plated brass body and slimline control lever.

Hand spray for sinks with Nylon flexible hose with integrated non-return valve.

F3/8” PEX flexibles .

Fixed via back nut.

Mixer with 30-year warranty.