**Swivelling column with retracting hand spray H. 200mm**

Reference: **1316**

Specification description

Swivelling column H. 195mm L. 215mm for mixers with retracting hand spray.

Column with retracting hand spray with 2 jet options with diverter (flow straightener/rain effect).

Securitouch thermal insulation prevents burns.

Column with smooth interior (reduces bacterial development).

BIOSAFE flexible hose reduces the spread of germs: transparent polyurethane flexible hose ensures replacement if biofilm is present, smooth interior and exterior.

Narrow flexible (interior Ø 6mm), low water volume.

Specific counterweight.

Body in chrome-plated brass.

Sink column with 30-year warranty.