**Mechanical basin mixer**

Single hole mechanical mixer H. 95mm L. 120mm

Hygiene control lever L. 150mm

Reference: **2721L**

Specification description

Deck-mounted mechanical basin mixer.

Single hole mixer with a curved spout H. 95mm L. 120mm fitted with hygienic flow straightener.

Spout suitable for fitting a BIOFIL point-of-use filter.

Ø 35mm ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors (reduces bacterial development).

Thermal shocks are easy to undertake without removing the lever or shutting off the water supply.

Flow rate regulated at 5 lpm.

Hygiene control lever L. 150mm.

Without pop-up waste.

F3/8" PEX flexibles.

Fixing reinforced via 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.

Also available with copper tails.