**BIOCLIP mechanical basin mixer**

Single hole removable mechanical mixer H.95mm L.120mm, Hygiene lever

Pop-up waste and stopcocks

Reference: **2820L**

Specification description

Deck-mounted mechanical basin mixer.

BIOCLIP mechanical mixer: mixer can be removed entirely for cleaning and disinfection.

Single hole mixer with spout H. 95mm L. 120mm fitted with a hygienic BIOSAFE nozzle.

Spout suitable for fiitting a BIOFIL point-of-use filter.

Ø 35mm ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume.

Flow rate limited to 5 lpm at 3 bar.

Hygiene control lever 150mm.

Ergonomic pop-up waste 1 1/4" made from brass.

Supplied with PEX flexibles F3/8" with stopcocks in chrome-plated brass.

Fixing reinforced by 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.

Also available with copper tails.