**Mechanical basin mixer**

Single hole mechanical mixer with swivelling spout H. 100mm L. 170mm

Mixer with Hygiene control lever

Reference: **2522L**

Specification description

Deck-mounted mechanical basin mixer.

Single hole mechanical mixer with swivelling spout H. 100mm L. 170mm fitted with a hygienic flow straightener.

Spout suitable for fitting a BIOFIL point-of-use filter.

Ø 40mm classic ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors.

Flow rate limited to 5 lpm at 3 bar.

Hygiene control lever L. 200mm.

PEX flexibles F3/8".

Fixing reinforced by 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.