**TEMPOMATIC MIX PRO electronic mixer**

Battery-operated

Swivelling, removable spout with smooth interior

Reference: **495257**

Specification description

Deck-mounted electronic basin mixer:

Independent IP65 electronic control unit.

Battery-operated with 123 6V Lithium batteries.

Flow rate pre-set at 4 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Shock-resistant infrared presence detection sensor.

Chrome-plated solid brass body with fixing reinforced by 2 stainless steel rods.

PEX flexibles with filters and solenoid valves M⅜".

360° swivelling spout with smooth interior (reduces bacterial development).

Removable spout for cleaning.

Anti-blocking security.

Side temperature control with ergonomic long lever and adjustable maximum temperature limiter.

Solenoid valves upstream of the mixing chamber.

Suitable for people with reduced mobility.

30-year warranty.