**TEMPOMATIC electronic tap with removable BIOCLIP spout**

Wall-mounted infrared tap with disposable spout

Mains supply

Reference: **20801T2**

Specification description

Wall-mounted electronic basin tap for mounting on panels.

Electronic tap with removable BIOCLIP spout.

Infrared sensor tap supplied with 1 removable, disposable spout made from recyclable Hostaform® L. 125mm.

Independent IP65 electronic control unit.

230/12V mains supply with transformer.

Spout and base with smooth interiors (reduces bacterial development).

Adjustable duty flush (pre-set at ~60 seconds every 24 hours after the last use).

Flow rate limited to 4 lpm at 3 bar.

Shock-resistant infrared presence detection sensor.

Separate sensor for mounting on panels.

M3/8" solenoid valve with integrated filter.

Ø 60mm chrome-plated brass base.

Anti-blocking security.

Recommended installation height: 110 - 200mm above the basin surface.

Electronic tap ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Electronic tap suitable for people with reduced mobility.

30-year warranty.

Two shut-off options:

 - standard mode: timed flow with automatic shut-off;

 - ON/OFF mode: user shuts off flow voluntarily or automatic shut-off after 30 minutes.

Thermal shocks are possible.

Install the sensor beside the tap in the ON/OFF mode.