**Shower riser rail with EP mechanical mixer**

Shower kit with EP Securitouch mixer

With offset STOP/CHECK connectors

Reference: **2739EPKIT**

Specification description

Shower riser rail with single control mechanical mixer.

Wall-mounted shower kit with SECURITHERM pressure-balancing shower mixer.

• Wall-mounted single control mixer with Securitouch thermal insulation to prevent burns.

Ø 40mm pressure-balancing (EP) ceramic cartridge with pre-set maximum temperature limiter.

Anti-scalding safety: HW flow is reduced if CW supply fails (and vice versa).

Constant temperature regardless of pressure or flow rate variations.

Body with smooth interior and low water volume.

Flow rate regulated at 9 lpm.

Chrome-plated brass body and sculptured control lever.

M1/2" shower outlet with integrated non-return valve.

Mixer with 2 offset STOP/CHECK wall connectors, M1/2" M3/4".

Filters and non-return valves.

• Sliding shower head holder (ref. 813) on a chrome-plated riser rail (ref. 821) with soap dish and flexible shower hose (ref. 836T1).

• Shower head retaining collar (ref. 830).

Mixer ideal for healthcare facilities, retirement homes, hospitals and clinics.

Mechanical mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.