**Copper tails**

M10 X 1, L. 365mm

2 per pack

Reference: **811610.2P**

Specification description

Soft-tempered copper tails M10 X 1, L. 365mm to supply mixer 2620.

Can be installed instead of PEX flexibles.

Improves efficiency of thermal shocks.

Supplied in packs of 2.

Pro tip: Don't forget to include non-return valves on the copper tails if the PEX flexibles to be replaced have integral non-return valves. Call our Technical Team for more information.