**Mechanical shower mixer**

Wall-mounted recessed mechanical mixer

With adjustable wall plate Ø 116mm

Reference: **2443**

Specification description

Wall-mounted, recessed, mechanical shower mixer with adjustable wall plate Ø 116mm.

Ø 40mm ceramic cartridge with pre-set maximum temperature limiter.

Solid control lever.

 Chrome-plated brass body.

Order a wall-mounted outlet (ref. 868121) or TONIC JET shower head (ref. 712000) or ROUND shower head (ref. 709000) to complete.

This mixer is not supplied with a waterproof housing. The installer must ensure that the recessing area is waterproof and allow a drainage point for any leaks or condensation.