**Mechanical mixer for remote control**

Mechanical mixer for retractible water taps

Mixer with sculptured lever

Reference: **2542**

Specification description

Mixer only, for deck-mounted independent control.

Ø 35mm ceramic cartridge with pre-set maximum temperature limiter.

 Sculptured control lever.

Chrome-plated brass body.

PEX flexibles F3/8".

Reinforced fixing via 2 stainless steel rods.

Sink mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

30-year warranty.