**Pre-rinse set with mixer**

With bib tap and swivelling telescopic spout

Black flexible with scale-resistant hand spray

Reference: **5625**

Specification description

Complete pre-rinse set with bib tap.

Single hole deck-mounted mixer with slimline control lever.

Suitable for intensive use in professional kitchens.

Supplied with F3/8" flexible hoses and non-return valves.

Bib tap with swivelling, tubular spout L. 200mm.

- 16 lpm full flow rate achieved within 90° turn.

- valve head with reinforced mechanism and ergonomic control.

Black hand spray with adjustable jet and 9 lpm flow rate at the outlet (ref. 433010).

Scale-resistant hand spray with shock-resistant tip.

Reinforced, food-grade black flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.