**TEMPOMATIC MIX 2 electronic mixer**

Electronic mains supply

Standard lever

Reference: **494000**

Specification description

Deck-mounted electronic basin mixer:

Independent IP65 electronic control unit.

230/12V mains supply with transformer.

Flow rate pre-set at 4 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Shock-resistant infrared presence detection sensor.

Chrome-plated brass body.

PEX flexibles with filters and solenoid valves M3/8".

Fixing reinforced by 2 stainless steel rods.

Anti-blocking security.

Side temperature control with adjustable maximum temperature limiter.

Solenoid valves are upsteream of the mixing chamber.

Suitable for people with reduced mobility.

30-year warranty.