**TEMPOMIX time flow mixer**

Single control, wall-mounted with fixed spout

Reference: **796000**

Specification description

Wall-mounted single control time flow basin mixer:

Soft-touch operation.

Temperature control and operation via the push-button.

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Solid chrome-plated brass body M¾".

Filters and non-return valves.

Adjustable maximum temperature limiter.

Fixed spout.

Chrome-plated metal control.

30-year warranty.