**TEMPOSTOP 2 time flow tap**

(AB) Anti-blocking model

Reinforced fixing

Reference: **702301**

Specification description

Deck-mounted time flow basin mixer:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Tamperproof scale-resistant flow straightener.

Chrome-plated brass body M½".

AB anti-blocking system: water will flow only when the push-button is released.

30-year warranty.