**Fixed spout with plate**

L. 170mm

Cross wall 165mm

Reference: **947157**

Specification description

Spout Ø 32mm, M½".

L. 170mm.

For cross wall installation for walls ≤ 165mm, with anti-rotating pin.

Threaded rod can be cut-to-size.

Chrome-plated solid brass.

Scale-resistant flow straightener regulated at 3 lpm.

30-year warranty.