**TEMPOSOFT 2 time flow shower valve**

Time flow

For panels, soft-touch operation

Reference: **749870**

Specification description

Time flow shower valve for panels:

TEMPOSOFT 2 M½" time flow valve for mixed water supply.

For panels or dry walls 7mm max.

Soft-touch operation.

Time flow ~30 seconds.

Flow rate pre-set at 6 lpm at 3 bar, can be adjusted.

Solid brass body.

Suitable for people with reduced mobility.

30-year warranty.

This model does not have a waterproof recessing box. The installer must ensure that the recessing area is waterproof and any leaks or condensates can drain away (see installation guide).