**GYM shower head**

Scale-resistant

Ceiling-mounted

Reference: **716000**

Specification description

Ceiling-mounted fixed shower head:

Flow rate 6 lpm at 3 bar.

Automatic flow rate regulation.

Scale-resistant and ligature-resistant nozzle with adjustable spray.

Chrome-plated solid brass.

Fixed with concealed blocking screw.

Systematically drains after use (no water retention or impurity deposits).

Inlets F½".

30-year warranty.