**PREMIX COMPACT Thermostatic mixing valve**

For mixed water 30 - 60°C

Nickel-plated brass body, 1 to 11 outlets, M¾"

Reference: **733020**

Specification description

Thermostatic mixing valve for mixed water distribution from 30 - 60°C:

For 1 to 11 sanitary points-of-use (depending on the flow rate).

Anti-scalding safety: immediate shut-off if cold or hot water supply fails.

Adjustable temperature from 30 - 60°C, can be blocked by the installer.

Brass body.

Filters and non-return valves.

Minimum flow rate to operate: from 5 - 33 lpm.

Thermal shocks are possible.

M¾".

40mm centres.

30-year warranty.