**TEMPOSTOP time flow urinal valve**

Time flow 3 seconds

Straight ½"

Reference: **777000**

Specification description

Exposed time flow urinal valve:

For standard, siphon action, or stall urinals.

For wall-mounted installation.

Time flow ~3 seconds.

Flow rate pre-set at 0.15 l/sec. at 3 bar, can be adjusted.

Compatible with rain water.

Chrome-plated brass body M½".

Wall plate.

Straight for in-line inlet.

30-year warranty.