**SECURITHERM shower panel**

Thermostatic shower panel with mixer with no non-return valves

Top inlets, shower head, flexible hose

Reference: **H9636**

Specification description

SECURITHERM shower panel made from anodised aluminium for wall-mounted exposed installation:

SECURITHERM sequential thermostatic shower mixer.

Thermostatic sequential mixer: opens and closes with cold water.

Mixer without non-return valves (reduces bacterial proliferation).

No risk of cross flow between the hot and cold water.

Sequential mixer with anti-scalding failsafe: shuts off automatically if cold water supply fails.

Cold water failsafe prevents cold showers: shuts off automatically if hot water supply fails.

Adjustable temperature control from cold water up to 39°C.

Maximum temperature limiter set at 39°C, can be adjusted.

Thermal shocks are possible.

Flow rate 9 lpm at 3 bar.

Sliding handset on a chrome-plated riser rail with removable flexible hose via rapid push-fit STOP connector.

Hygiene control lever L. 100mm.

Top inlets with M1/2" stopcocks.

Concealed fixings.

Filters.

Shower panel ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Suitable for people with reduced mobility.

Shower panel with 30-year warranty.