**Pre-rinse set with mixer**

With bib tap and swivelling telescopic spout

Black flexible and scale-resistant hand spray

Reference: **5632**

Specification description

Complete pre-rinse set with bib tap suitable for intensive use in professional kitchens.

Deck-mounted single hole mixer with:

- valve heads with reinforced mechanisms and ergonomic control levers.

- F3/8" flexibles and non-return valves.

- reinforced fixing via 2 threaded rods with back-nuts.

Bib tap with swivelling, tubular spout L. 200mm.

- 20 lpm full flow rate achieved within the first 90°.

- valve head with reinforced mechanism and ergonomic control lever.

Black hand spray with adjustable jet and 9 lpm flow rate at the outlet (ref. 433010).

Scale-resistant hand spray with shock-resistant tip.

Black, reinforced, food-grade flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.