**Wall-mounted twin hole mixer - 60 lpm**

Swivelling over spout L. 200mm

For a clear work surface

Reference: **5647T2**

Specification description

Wall-mounted twin hole mixer with swivelling, tubular over spout Ø 22mm L. 200mm.

 Star-shaped flow straightener.

Water-free, guided valve heads with reinforced mechanisms.

Shock-resistant, ergonomic ball levers.

Flow rate 60 lpm at 3 bar achieved within 90°.

Full flow rate 90 lpm at 3 bar.

Spout with smooth interior.

One-piece body and spout made from chrome-plated brass.

M1/2" M3/4" offset connectors supplied with escutcheons.

Suitable for disposal sinks.

30-year warranty.