**Stainless steel BIOCLIP spout**

Spout L. 77mm Ø28mm for mixers with removable spouts

2 per pack

Reference: **20003**

Specification description

Removable stainless steel BIOCLIP spout L. 77mm, Ø 28mm for easy cleaning/descaling of the interior or autoclaving.

Fitted with a hygienic flow straightener, suitable for fitting a point-of-use BIOFIL filter.

Spout with smooth interior reduces bacterial development.

The second spout enables continuous use during cleaning/descaling of the first spout.

Suitable for all mixers and taps with BIOCLIP spout.

2 per pack.