**Towel rail**

Ø 20mm, 2 rails

Polished satin 304 stainless steel

Reference: **510790S**

Specification description

Towel rail for bathrooms.

Twin rail designer towel rail.

Robust model.

Ø 20mm and Ø 16mm rails, length 600mm.

Bacteriostatic 304 stainless steel with polished satin finish.

Wall-mounted towel rail with concealed fixings.

30-year warranty.