**TEMPOMIX time flow shower mixer**

Single control time flow

Recessed, Ø 195mm wall plate

Reference: **790925**

Specification description

Recessed time flow shower kit:

Chrome-plated Ø 195mm wall plate.

Standard recessing housing.

Recessing depth adjustable from 28 - 43mm.

TEMPOMIX ¾" single control mixer.

Ligature-resistant collar.

Temperature control and operation via the push-button.

Maximum temperature limiter (can be adjusted by the installer).

Time flow ~30 seconds, soft-touch operation.

Flow rate 12 lpm at 3 bar.

M½" connectors for Ø 15mm copper tubes.

Integrated non-return valves and filters.

Chrome-plated metal control.

30-year warranty.

As this model does not come with waterproof recessing housing the installer must ensure the watertightness of the recessing area and allow for run-off of leaks and condensation (see installation guide).