**TEMPOSTOP**

For hand washbasins

With button

Reference: **748626**

Specification description

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, adjustable from 1.4 to 6 lpm.

Rough cast solid brass body and chrome-plated push-button.

Inlet M1/2".

To be placed behind hand washbasin wall plate.

30-year warranty.