**TEMPOMIX 3 time flow shower kit**

Time flow single control

Exposed TONIC JET shower head, mixer, soft-touch

Reference: **794450**

Specification description

Exposed time flow shower kit:

TEMPOMIX 3 single control mixer ¾", top outlet.

For wall-mounted, exposed installation.

Temperature control and operation via the push-button.

Maximum temperature limiter (can be adjusted by the installer).

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant TONIC JET shower head with automatic flow rate regulation.

Chrome-plated solid brass.

Integrated filters and non-return valves.

Chrome-plated metal push-button.

Shower column Ø 16mm with reinforced collar (fixing plate and screws included).

M½" offset connectors for 130 - 170mm centres.

Suitable for people with reduced mobility.

30-year warranty.