**PREMIX NANO thermostatic mixing valve**

For mixed water from 34 - 60°C

Nickel-plated body, M½" Ø 15mm

Reference: **732115**

Specification description

Hot water thermostatic mixing valve for mixed water distribution from 34 - 60°C:

For 1 - 2 taps or 1 shower.

Anti-scalding safety: immediate shut-off if cold or hot water fails.

Temperature pre-set at 38°C, can be adjusted by the installer from 34 - 60°C.

Brass body.

Filters and non-return valves.

Minimum flow rate to operate: 3 lpm.

Thermal shocks are possible.

Nickel-plated brass body M½" inlets and Ø 15mm conical outlets.

30-year warranty.