**Floor trap**

For tiled or concrete floors

100x100mm

Reference: **682001DE**

Specification description

Floor trap for hard floors (tiles or concrete floors) with adjustable height:

Flow rate 36 lpm (standard).

Water level 50mm.

100 x 100mm bright polished stainless steel grid.

Ø 50mm horizontal outlet integrated into the height of the floor trap (saves height and space in all directions).

Integrated waterproof collar to seal waterproof membrane.

Withstands high temperatures: 60°C continuous, 85°C peak.

Plunger with handle: easy to grip and easy to clean.

Smooth PVC body (prevents build-up of impurities).

Classified non-flammable (American certification UL94).

110mm high, adjusts up to 80mm with extension.

Grill fixed with two stainless steel screws.

30-year warranty.