**Mechanical shower panel**

Mechanical

Top inlet Ø 15mm, fixed shower head, aluminium

Reference: **79130015**

Specification description

Mechanical shower panel with single control mixer and fixed shower head:

Anodised aluminium shower panel for wall-mounted, exposed installation.

Top inlet via in-line stopcocks and conical Ø 15mm inlets.

Non-time flow mechanical mixer.

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation.

Concealed fixings.

Filters.

Suitable for people with reduced mobility.

30-year warranty.