**Floor trap**

For soft or vinyl floors

Ø 114mm

Reference: **683002UK**

Specification description

Adjustable height floor trap for soft or vinyl floors:

Flow rate 36 lpm (meets standards).

Water level 50mm.

Bright polished stainless steel grid Ø 114mm.

Ø 43mm horizontal outlet integrated into the height of the floor trap (saves height and space in all dimensions).

Integrated waterproof plate to seal waterproof membrane.

Withstands high temperatures: 60°C continuous, 85°C peak.

Plunger with handle: easy to grip and easy to clean.

Smooth PVC body (prevents build-up of impurities).

Classified non-flammable (American certification UL94).

Height adjusts up to 85mm with extension.

Grid fixed by two stainless steel screws.

30-year warranty.