**SECURITHERM time flow shower panel**

Thermostatic time flow

Top inlet, fixed head, stainless steel, soap dish

Reference: **79230415**

Specification description

Thermostatic time flow shower panel:

Large model satin stainless steel shower panel for wall mounted, exposed installation.

Top inlet via in-line stopcocks and Ø 15mm conical inlets.

SECURITHERM thermostatic shower mixer.

Adjustable temperature control from cold water up to 41°C.

Anti-scalding safety: automtaic shut-off if cold or hot water supply fails.

Thermal shocks are possible.

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant, fixed, ROUND shower head with automatic flow rate regulation.

Integrated soap dish.

Concealed fixings.

Filters and non-return valves.

Suitable for people with reduced mobility

30-year warranty.