**Wall-mounted TRAPEZ washbasin**

Polished satin 304 stainless steel

With central tap hole Ø 35mm

Reference: **121270**

Specification description

Wall-mounted washbasin, 600x505mm.

Washbasin suitable for people with reduced mobility.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

With central tap hole Ø 35mm.

Supplied with 1¼" waste.

Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 5.5kg.

30-year warranty.

[Formerly ref: 3411270008]