**CANAL wall-mounted wash trough**

Polished satin 304 stainless steel - L. 600mm

Without tap hole

Reference: **120240**

Specification description

Wall-mounted wash trough for wall-mounting, 1 service - 600mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 0.8mm for the bowl, 1.5mm for surround and fixing brackets.

Easy to install: no joint concealers to install, lightweight trough.

Water control can be wall-mounted or deck-mounted.

Drainage on the right.

Without tap hole.

Supplied with 1½" waste. Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14296.

Weight: 4.9kg.

30-year warranty.

Possible to add a bacteriostatic 304 stainless steel splashback (ref. 0011800001).

[Formerly ref: 0211240015]