**Floor-standing SXL hand washbasin**

Polished satin 304 stainless steel - Foot-operated

With integrated tap

Reference: **180300**

Specification description

Floor-standing, foot-operated hand washbasin.

Bacteriostatic 304 stainless steel. Polished satin finish. Stainless steel thickness: 0.8mm.

Supplied with swan neck spout and time flow tap with 7 second time flow.

Easy to maintain: access panel at the front.

Supplied with 1¼" waste.

Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 10kg.

30-year warranty.

[Formerly ref: 3410300003]