**SHA XS squat WC pan**

Polished satin 304 stainless steel - recessed - with trap

1 spreader

Reference: **113720**

Specification description

Floor-recessed squat WC pan, 500 x 325 x 600mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness 1.2mm.

One-piece pressed WC bowl, seam-free for easy maintenance and better hygiene.

Bowl shape suitable for male and female use.

Non-slip foot area.

Waste outlet: Ø 100mm.

Flushing system with one 304 stainless steel spreader.

Supplied with stainless steel trap welded to squat WC pan.

Weight: 7kg.

30-year warranty.

[Formerly ref: 0113370020]