**LP individual urinal**

Polished satin 304 stainless steel - L. 600mm - Floor-standing

Reference: **130300**

Specification description

Floor-standing urinal, 600 x 1020 x 300mm.

Bacteriostatic 304 stainless steel.

Polished satin stainless steel. Stainless steel thickness: 1.2mm

Rear water inlet.

Supplied with 1 stainless steel rinser and a flexible hose.

Water saving: optimal rinsing with 0.1 L/sec. per service i.e. 0.3L per use.

Central drainage.

Waste outlet 1½". Supplied with waste and integrated trap (ref. 785000).

Easy to install and maintain thanks to access panels with theft prevention TORX security screws.

Weight: 15.2kg.