**Wall-hung trough urinal**

Polished satin 304 stainless steel - L. 1800mm

Reference: **130110**

Specification description

Wall-hung trough urinal, 1800 x 575 x 275mm.

Bacteriostatic 304 stainless steel. Polished satin finish.

Stainless steel thickness: 1.2mm.

Top water inlet F½".

Supplied with 1 stainless steel spreader pipe (perforated horizontal pipe) for optimum rinsing of urinal surface.

Water savings: optimal rinsing with 0.1 L/sec. per service i.e. 0.3L per use.

Drainage on the right. Waste outlet 1½".

Supplied with fixing elements.

Without trap.

Possible to add one or more bacteriostatic 304 stainless steel dividers (ref. 100900). Fix directly onto the urinal in the desired location.

Installation advice: if you wish to install 2 urinals side by side, we recommend ordering one urinal with drainage on the left and one with drainage on the right.

Weight: 24.8kg.