**LISO XL urinal divider for wall-mounting**

Polished satin 304 stainless steel - H. 950mm

Reference: **100600**

Specification description

Urinal divider for wall-mounting.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.5mm

Smooth surface and rounded edges.

Concealed fixings.

Supplied with fixing elements.

Weight: 13kg

[Formerly ref: 0011600000]