**SECURITHERM shower panel**

Thermostatic time flow dual control

Concealed inlet, fixed and handheld shwr head, alu

Reference: **792330**

Specification description

SECURITHERM dual control thermostatic time flow shower panel:

Anodised aluminium shower panel for wall-mounted, exposed installation.

With concealed inlet via flexibles, M½".

SECURITHERM thermostatic shower mixer.

Adjustable temperature control from cold water up to 38°C with 1st limiter set at 38°C and 2nd limiter set at 41°C.

Anti-scalding failsafe: automatic shut-off if cold water fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Thermal shocks are possible.

Soft-touch operation.

Chrome-plated, tamperproof, scale-resistant, fixed, ROUND shower head with automatic flow rate regulation at 6 lpm at 3 bar.

Handset with removable flexible via push-fit rapid STOP connector and wall support supplied.

2x ~30 second time flow valves to control fixed ROUND shower head and handset on flexible hose.

Concealed fixings.

Filters and non-return valves.

Time flow shower panel suitable for people with reduced mobility.

30-year warranty.