**Aluminium shower panel with SECURITHERM sequential mixer**

Sequential thermostatic

Concealed inlet, fixed shower head, aluminium

Reference: **H9634**

Specification description

Anodised aluminium shower panel for wall-mounted exposed installation:

SECURITHERM sequential thermostatic mixer (non time flow).

Adjustable temperature control from cold water up to 39°C; maximum temperature limiter set at 39°C, can be adjusted.

Anti-scalding safety: automatic shut-off if cold water supply fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Thermal shocks are possible.

Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation at 6 lpm at 3 bar.

Hygiene control lever L. 100mm.

Concealed supply via M1/2" flexibles.

Concealed fixings.

Filters.

Suitable for people with reduced mobility.

30-year warranty.