**Aluminium shower panel with SECURITHERM sequential mixer**

Sequential thermostatic

Concealed inlet, handset, aluminium

Reference: **H9635**

Specification description

Anodised aluminium shower panel for wall-mounted, exposed installation:

SECURITHERM sequential thermostatic mixer (non time flow).

Adjustable temperature control from cold water up to 39°C; maximum temperature limiter set at 39°C, can be adjusted.

Anti-scalding failsafe: automatic shut-off if cold water fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Thermal shocks are possible.

Flow rate 9 lpm at 3 bar.

Sliding handset on a chrome-plated riser rail with removable flexible hose via rapid push-fit STOP connector.

Hygiene control lever L. 100mm.

Concealed supply via M1/2" flexibles.

Concealed fixings

Filters.

Suitable for people with reduced mobility.

30-year warranty.