**TEMPOMATIC MIX 4 electronic mixer - Kit 2/2**

Mains supply (recessed unit)

Recessed, L. 160mm, integrated electronics

Reference: **493400**

Specification description

Wall-mounted electronic basin mixer, kit 2/2:

230/6V recessed mains supply.

Reduced-stagnation solenoid valve and electronic unit integrated into the body of the mixer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Duty flush (~60 seconds every 24 hours after last use).

Presence detection sensor at the end of the spout optimises detection.

Chrome-plated stainless steel body L. 160mm.

Cap fixed in place by 2 concealed screws.

Stopcocks.

Wall-mounted.

Recessed inlets ½".

Top or bottom supply.

Anti-blocking security.

Side temperature control with adjustable maximum temperature limiter.

Suitable for people with reduced mobility.

30-year warranty.

Order with nanny joint for recessed inlet, reference: 484012