**Shower riser kit with EP mechanical mixer**

Shower riser rail with pressure-balancing mixer

With STOP/CHECK connectors

Reference: **2239EPKIT**

Specification description

Shower riser rail with single control mechanical mixer.

• Wall-mounted shower kit with EP shower mixer.

Ø 40mm ceramic cartridge with pressure-balancing (EP) with pre-set maximum temperature limiter.

Total anti-scalding safety: HW flow rate is reduced if CW supply fails (and vice versa).

Stable temperatures regardless of pressure and flow rate variations.

Flow rate regulated at 9 lpm.

Chrome-plated brass body, operated by a sculptured control lever.

M½" shower outlet with integrated non-return valve.

Mixer with 2 offset STOP/CHECK wall connectors M1/2" M3/4" ideal for hospitals.

Filters and non-return valves.

• Sliding shower head (ref. 811) on chrome-plated riser rail (ref. 820) with soap holder and flexible hose (ref. 834T1).

Shower riser rail ideal for healthcare facilities, nursing homes, hospitals and clinics.

Suitable for people with reduced mobility.

30-year warranty.